|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Water level | | Time | | Name Uruguayan wells and Flumes Data: 11/01/19 | | | | |
| Station | Actual mm | Module mm | Actual | Module |  | | | | |
| Flumes |  |  |  |  |  | | | | |
| V1 |  | 0.41 | 15:15 |  | OBS.T= 81.8°F Rule White:30 batería bien | | | | |
| S 1 |  |  | 15:00 |  |  | | | | |
| E1  (auxiliar) |  |  | 15:05 |  |  | | | | |
| V2 |  | 0.32 | 16:33 |  | OBS.: T=73.5°F Rule white:80 batería bien 96% | | | | |
| S2 |  |  | 16:22 |  |  | | | | |
| E2  (auxiliar) |  |  | 16:28 |  |  | | | | |
| **Sampler** |  |  |  |  | # Smp | Flow, m3/s | Smp Flow, m3 | Tot Flow, m3 | Comments |
| SMP1 | 55 | 0.002 | 14:54 |  | 57 | 0.000 | 1054 | 68550 | Error have ocurred during in the program..AJUSTE MANUAL NIVEL DE LA REGLA. PURGAMOS |
| SMP2 |  | 0.069 | 16:20 |  | 91 | 0.007 | 137.2 | 109062 | PUERGAMOS |
| **Wells** |  |  |  |  |  | | | | |
| N1 |  |  |  |  |  | | | | |
| N1.1 |  |  |  |  | Manual Well | | | | |
| N1.2 |  |  |  |  | Manual Well | | | | |
| N1.3 |  |  |  |  | Manual Well | | | | |
| N2 |  |  |  |  |  | | | | |
| N3 |  |  |  |  |  | | | | |
| N4 |  |  |  |  |  | | | | |
| N5 |  |  |  |  |  | | | | |
| N5.1 |  |  |  |  | Manual Well | | | | |
| N5.2 |  |  |  |  | Manual Well | | | | |
| N5.3 |  |  |  |  | Manual Well | | | | |
| N6 |  |  |  |  |  | | | | |
| Rain |  |  |  |  |  | | | | |
| RV1 |  |  |  |  | Manual Rain Gauge nears the flume V1 | | | | |
| R2 |  |  |  |  | Manual Rain Gauge nears the road | | | | |
| R3 |  |  |  |  | Manual Rain Gauge nears the road | | | | |
| R4 |  |  |  |  | Manual Rain Gauge nears the house | | | | |
| R1 |  |  | 16:26 |  | Manual Rain Gauge nears the flume V2. | | | | |
| Weather |  |  |  |  |  | | | | |
| EM |  |  | 17:09 |  |  | | | | |
| WS |  |  | 17:13 |  | T= 84.2°F - H.R=69.7 % - 17.2 intensidad de luz.-73.46°F punto de Rocio-70% bateria. | | | | |
|  |  |  |  |  |  | | | | |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Water level | | Time | | Name Uruguayan wells and Flumes Data:**11/01/19** | | | | |
| Station | Actual mm | Module mm | Actual | Module | Comments | | | | |
| Flumes |  |  |  |  | **Note : Actual stage equals 0.4 times Observed Stage** | | | | |
| V3 |  | 2.21 | 14:30 |  | Measuring vertical water:6 cm Rule white:160. 96% bateria | | | | |
| Bar3 |  |  | 14:17 |  | T= Promedio 3 muestras agua: | | | | |
| V3p |  |  | 14:15 |  | OBS.: T= | | | | |
| V4 |  | 0.39 | 12:00 |  | Measuring vertical water: 11 cm Rule white: 340 .96%bateria. | | | | |
| V4p |  |  | 11:39 |  | OBS. T= Promedio 3 muestras agua: | | | | |
| Bar |  |  | 11:41 |  | T= |  |  |  |  |
| **Sampler** |  |  |  |  | # Smp | Flow, m3/s | Smp Flow, m3 | Tot Flow, m3 | Comments |
| SMP3 | 45/57 | 0.045 |  |  | 24 | 0.007 | 491.4 | 18710 | 0.02mps-signal 0%  Error have occurred durin in the program.  PURGAMOS |
| SMP4 | 80/90 | 0.098 | 11:45 |  | 28 | 0.015 | 376 | 22020 | Signal:15%-spectrum:93%.  PURGAMOS |
| **Wells** |  |  |  |  |  | | | | |
| N7 |  |  |  |  |  | | | | |
| N8 |  |  |  |  |  | | | | |
| N8.1 |  |  |  |  | Manual Well | | | | |
| N8.2 |  |  |  |  | Manual Well | | | | |
| N9 |  |  |  |  |  | | | | |
| N10 |  |  | 17:32 |  | Vaciamos el pozo para sacar restos de avejas. | | | | |
| N10.1 |  |  |  |  | Manual Well | | | | |
| N10.2 |  |  |  |  | Manual Well | | | | |
| N11 |  |  |  |  |  | | | | |
| N12 |  |  |  |  |  | | | | |
| N12.1 |  |  |  |  | Manual Well | | | | |
| N12.2 |  |  |  |  | Manual Well | | | | |
| N12.3 |  |  |  |  | Manual Well | | | | |
| N13 |  |  |  |  |  | | | | |
| Rain |  |  |  |  |  | | | | |
| R5 |  |  |  |  | Manual Rain Gauge near trees | | | | |
| R6 |  |  |  |  | Manual Rain Gauge near field | | | | |
| R7 |  |  | 11:38 |  |  | | | | |